AuboStudio SDK 0.6.3

Public 成员函数 | 所有成员列表
arcs::aubo_scope::RegisteredCapabilities类 参考abstract

`#include <registered_cpabilities.h>`

## Public 成员函数
virtual | ~RegisteredCapabilities ()=default
virtual WidthCapabilityPtr | getWidthCapability ()=0
virtual GripForceCapabilityPtr | getGripForceCapability ()=0
virtual SpeedCapabilityPtr | getSpeedCapability ()=0
virtual GripVacuumCapabilityPtr | getGripVacuumCapability ()=0

## 详细描述

Each of the individual grippers/zones available in a multi-gripper device supports all capabilities that has been registered, i.e. all the individual grippers have the exact same set of capabilities. This interface gives access to all registered capabilities, such as the width capability (see {}), speed capability (see SpeedCapability}), etc. This enables dynamic adjustment of capability properties, including the value range and default values, exclusively per individual gripper (independently of the other grippers).

This interface is only relevant if the multi-gripper capability has been registered (using the method double, double, double, Length.Unit)).

Each capability must be registered using the {} interface (when GripperContribution#configureGripper(GripperConfiguration, GripperAPIProvider)} is called) before they can be accessed using this interface.

NOTE: If an update of the properties of a capability needs to apply for all individual grippers, it is more convenient to perform the adjustment simultaneously for all grippers using the capability instance (e.g. WidthCapability) returned when the capability was registered (with the GripperCapabilities interface).

在文件 registered_cpabilities.h 第 49 行定义.

## 构造及析构函数说明

## ◆ ~RegisteredCapabilities()

virtual arcs::aubo_scope::RegisteredCapabilities::~RegisteredCapabilities | ( |  | ) |
| virtual default

## 成员函数说明

## ◆ getGripForceCapability()

virtual GripForceCapabilityPtr arcs::aubo_scope::RegisteredCapabilities::getGripForceCapability | ( |  | ) |
| pure virtual

Access the grip force capability interface which allows for dynamic adjustments of the capability properties exclusively for this specific individual gripper (independently of the other grippers), including the value range and default value.

This is only valid, if the force capability has been registered (using the method double, double, Force.Unit)).

返回
  The grip force capability for this individual gripper

异常

  UnsupportedOperationException | if the gripper has not registered the force capability

## ◆ getGripVacuumCapability()

virtual GripVacuumCapabilityPtr arcs::aubo_scope::RegisteredCapabilities::getGripVacuumCapability | ( |  | ) |
| pure virtual

Access the grip vacuum capability interface which allows for dynamic adjustments of the capability properties exclusively for this specific individual gripper (independently of the other grippers), including the value range and default value.

This is only valid, if the vacuum capability has been registered (using the method double, double, Pressure.Unit)).

返回
  The grip vacuum capability for this individual gripper

异常

  UnsupportedOperationException | if the gripper has not registered the vacuum capability

## ◆ getSpeedCapability()

virtual SpeedCapabilityPtr arcs::aubo_scope::RegisteredCapabilities::getSpeedCapability | ( |  | ) |
| pure virtual

Access the speed capability interface which allows for dynamic adjustments of the capability properties exclusively for this specific individual gripper (independently of the other grippers), including the value range and default value.

This is only valid, if the speed capability has been registered (using the method double, double, double, Speed.Unit)).

返回
  The speed capability for this individual gripper

异常

  UnsupportedOperationException | if the gripper has not registered the speed capability

## ◆ getWidthCapability()

virtual WidthCapabilityPtr arcs::aubo_scope::RegisteredCapabilities::getWidthCapability | ( |  | ) |
| pure virtual

Access the width capability interface which allows for dynamic adjustments of the capability properties exclusively for this specific individual gripper (independently of the other grippers), including the value range and default value.

This is only valid, if the width capability has been registered (using the method double, double, double, Length.Unit)).

返回
  The width capability for this individual gripper

异常

  UnsupportedOperationException | if the gripper has not registered the width capability

该类的文档由以下文件生成:

- include/aubo_caps/contribution/driver/gripper/capability/registered_cpabilities.h